**VEHICLE AND TRAILER INSPECTION CHECKLIST**

|  |  |  |  |
| --- | --- | --- | --- |
| Inspector: |  | Date: |  |
|  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CAR / VAN / TRUCK | | | | |
| Vehicle: |  | Mileage: | |  |
|  | |  |  |  |
| ITEM INSPECTED | | OK | REPAIR | COMMENTS |
| Tires, including wear and air pressure | |  |  |  |
| Engine fluid levels | |  |  |  |
| Fuel, coolant and oil leaks | |  |  |  |
| Belts and hoses | |  |  |  |
| Brakes | |  |  |  |
| Lights including turn signals/brakes | |  |  |  |
| Horn, gauges and controls | |  |  |  |
| Steering | |  |  |  |
| Windshield, wipers, side and rear view mirrors | |  |  |  |
| Seat belts | |  |  |  |
| Fire extinguisher and First Aid Kit | |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TRAILER | | | | |
| Trailer: |  | | |  |
|  | | | | |
| ITEM INSPECTED | | OK | REPAIR | COMMENTS |
| Pin securing ball mount to receiver is intact | |  |  |  |
| Hitch coupler is secured | |  |  |  |
| Spring bar hinges and safety clips in place | |  |  |  |
| Safety chains properly attached | |  |  |  |
| Electrical wiring and plugs in good condition | |  |  |  |
| Reflectors and required signs in good condition | |  |  |  |
| Brake, signal and plate lights work | |  |  |  |
| Tires, including wear, air pressure and lug nuts | |  |  |  |
| Trailer in overall good condition | |  |  |  |
| Load is secured and weight even | |  |  |  |
| Check visibility in tow vehicle mirrors | |  |  |  |
| Know weight, height and width limits for load | |  |  |  |